{"text_format":"3","workbook":"xls","n_sheets":4,"sheets":["Sheet4","Sheet1","Sheet2","Sheet3"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet4","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet1","index":1,"n_rows":13,"n_cols":5,"rows_kept":13,"merged":[[0,0,0,4],[1,0,1,3],[12,0,12,4]],"flags":["formulas_cached_only"]}
["创建节水型学校建设项目清单"]
["工程名称:毕节市财贸学校创建节水型学校建设项目"]
["序号","工程或费用名称","单位","数量","备注"]
["一","改造","项",1]
[1,"雨水收集","项",1,"新建8m³雨水收集池（地埋），接学校雨水管网，经增压泵增压用于喷灌或学校卫生间使用（考评分5分）"]
[2,"灰水收集","项",1,"教学楼公共厕所洗手台用水接入灰水收集箱用于下层卫生间冲厕使用（考评分5分）"]
[3,"喷灌","项",1,"在校区内选择适合的一片或两片绿化进行建设"]
[4,"节水宣传标语","项",1,"校区内用水设施、器具旁、公共场所张贴节水宣传"]
[5,"器具改造","项",1,"非节水型设备更换"]
[6,"卫生间管网改造","项",1,"此项为灰水收集用于下层卫生间产生的改造"]
[7,"计量设施加装","项",1,"新增喷灌及学校单元楼目前缺少的水表，安装水表的同时装阀"]
["二","创建节水型学校技术服务","项",1,"含水平衡测试及创建节水型学校申报工作"]
["说明： 此清单为初步概算，具体实施价以实际发生量为准。"]

{"sheet":"Sheet2","index":2,"n_rows":9,"n_cols":9,"rows_kept":9,"flags":["formulas_cached_only"]}
["主楼DN100","下口宽","上口宽","高度","青石板厚","C15垫层","中砂层",null,"人行道面积"]
[null,0.375,null,1.05,0.05,0.1,null,null,1.005]
[]
[]
[]
[]
[]
[]
[{"$nulls":7}," "]

{"sheet":"Sheet3","index":3,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}